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Legend Hobby B-17 Navigation Lights

The Legend Hobby B-17 Navigation Light Set is designed to plug into any spare channel on your receiver, and provides two Wingtip Navigation Lights, a Tailcone Light, an Anti-Collision Strobe, a Simulated Rotating Beacon, and two Landing Lights, most of which are switchable from the transmitter.  It also features 6 different strobe/beacon patterns that can be selected by the small push-button switch located on the main circuit board.  The 6 patterns change the speed of the rotating beacon and the number of times the strobe blinks between pauses.  The last pattern chosen is stored to the circuit’s memory so that it retains the setting even after the plane’s battery is removed.
	In order to allow the various outputs to be switched from the transmitter, the circuit should be plugged into a proportional channel, typically channel 6 or higher.  Avoid using the gear channel unless you are certain that your radio allows proportional control of the gear channel.  Adjust the ATV or End Point of the channel you choose to 90-95% in each direction, but no more than 100%.  The channel you select should be one that can be controlled with a knob or slider, and/or a 3-position switch.  The Custom All-in-One Navigation Light Set has 3 modes, which respond to approximately the programmable channel mixes shown below:


Mode #1:  Wingtip (Red/Green) Lights On-----0% (-100%)
Mode #2:  Wingtip, Rotating Beacon and Strobe On---- greater than 25% (-50%)
Mode #3:  All Lights, including Landing Lights On---- greater than 50% (0% or channel center)


          Plug the circuit into the receiver, and rotate the knob fully counter-clockwise (CCW).  All lights should be Off.  If they are not, reverse the channel in the transmitter’s programming.  As you advance the channel you selected, you should see the lights come on in the order of the 3 modes above.  If you wish, you can use a 3-position switch and programmable mixes to control the 3 modes.


(continued on back)
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The 6 available patterns can be selected via the small pushbutton switch on the main circuit board.  (See picture above).  The 6 patterns are listed below:

#1:  Single-blink Strobe/ Slow Beacon speed            #4: Double-blink Strobe/ Slow Beacon speed
	#2:  Single-blink Strobe/ Medium Beacon speed       #5: Double-blink Strobe/ Medium Beacon speed
#3:  Single-blink Strobe/ Fast Beacon speed             #6: Double-blink Strobe/ Fast Beacon speed

Once you’ve scrolled through all 6 patterns, the next button press will cause all the LEDs to fade up and down, indicating you’ve gone through the available patterns and are about to re-start at pattern #1.  About 15 seconds after your last selection, the circuit will save that pattern to its memory so it will start in that pattern every time, unless (or until) it is changed again.


If you have any questions or problems, don’t hesitate to contact me.  ENJOY!
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